시    방   서

<HEN-30B>

㈜ 루 먼 텍

서울특별시 금천구 가산디지털1로 131

(가산동,BYC하이시티지식센터A동11층)

TEL. 02-6947-7400  FAX.02-6947-7440

1. 적용범위 및 분류

1.1 적용범위

본 규격서는 조달청에 다수공급자물품계약에 의해 처리되는 통신용변조기에 대하여 적용한다.

1.2 분류

물품분류번호	물품식별번호	규격명	용도	인도조건
32101528	23021664	HEN-30B	HD, SD encoding 및 8VSB Modulator	현장설치도

2. 적용자료 및 문서

조달청 내자공고 제 제 20160919822-00호 적용.

번호	인증명	인증번호	발급기관
3	방송통신기자재 적합인증	MSIP-CTM-KLU-EN3	국립전파연구원

3. 필요조건

3.1 재료

품명	식별번호	규격명	주재료명	주재료 공급자	원산지
통신용변조기	23021664	HEN-30B	CASE	기드온	한국
			PCB	은성일렉콤	한국

3.2 형태

19 표준 렉에 장착이 가능한 제품의 형태로써 제품의 전원 투입 상태 및 조작상태를

전면의 LCD 창을 통하여 확인 가능하도록 구성한다

3.3 제조 및 가공

원재료입고, 조립가공, 품질검사, 물류창고

3.4 기능 및 성능

1. HEN-30B

본 기기는 HD encoder와 Modulator가 결합된 HD Encodulator로서 공중파급 Full HD

Encoder와 디지털 방송 변조기(ATSC)가 일체형으로 만들어진 장비입니다.

다양한 비디오/오디오 인터페이스(HDMI, HD-SDI, RCA-L/R,IP)를  제공하며 CATV,

MATV, 학교 교육 방송, 사내 방송, 교회, 아파트, 발전소, 박물관, 백화점등 방송 시설이

필요한 매우 다양한 곳에서 사용할 수 있는 목적 장비입니다.

6. 재원 및 제품 구성

6.1 용도

영상 음성신호를 RF 신호로 변조하여 지정의 채널로 출력합니다..

6.2 발주재원

Type	HD Encoder + 8VSB Modulator
Inputs	SD/HD-SDI,BNC75Ω1ea
	HDMI 1.4a 1ea (HDCP supported)
	Analog Stereo Audio (Left/Right), RCA 2ea
VideoResolutions	1920x1080 @ 60p, 59.94p, 50p Automatic Convert to Interlaced Format
	1920x1080 @ 60i, 59.94i, 50i
	1280x720 @ 60p, 59.94p, 50p
	720x480 @ 59.94i (NTSC)
	720x575 @ 50i(PAL)
	Resolution detect and automatic/manual change support
TSMux& System	System Delay: 150ms, 200ms, 350ms,650ms
	TS Bit-rate: 4.5~25 Mbps
	Editable TS ID, PMT/PCR/Video/Audio PID
VideoEncoder	MPEG2, H.264
	MPEG2 HD/SD (MP@HL/MP@ML), H.264 HD/SD (HP@L4/HP@L3)
	Bit Rate: (MPEG2) 5Mbps ~ 22 Mbps, (H.264) 3.5Mbps ~ 22Mbps
	Closed Caption Support
AudioEncoder	MP1L2, Dolby AC3, AAC-LC, HE-AACv2 (Stereo)
	Bit-rate: 192~384 Kbps (HE-AACv2: 32~96Kbps)
	Sample Rate: 48KHz
	Audio Delay: 0~400ms
	Volume Control: 100%~500%
PSIPGenerator	MGT, TVCT Generation Enable/Disable
	Short name, major and minor channel number setting
ASIOutput	Connector:BNC75Ω1ea
	PacketSize:188Bytes
	TSBitRate:19.392Mbps
RFOutput	Modulation:ATSC(8VSB)
	Connector:F-Type75Ω1ea
	OutputLevel:+2~-18dBm(0.5dBStep)
	CenterFrequencyRange:40~999MHz
	MER:>36dB
	Spurious:60dBc(RelativetoOutputLevel)
	PhaseNoise:VHF110dBc@20kHz,UHF95dBc@20kHz
IPOutput (*Option)	Ethernet : 10/100Base-T, half/full duplex
	MaximumTransmissionUnit : 1464~1472 MTU
	Streaming Protocol : MPEG2-TS/UDP
	Transport Protocol : UDP, Unicast or Multicast
	IGMPv1, IGMPv2 support
Management	FrontPanel:4-linetextLCD,6buttons,StatusLED(RGB)
	RearUSBPort:GUI,FirmwareUpdate
Physical	Dimension:44(H)X483(W)X240(D)(excludingconnectors)
	OperationTemperature:0~45℃
	Weight:2Kg
	PowerConsumption:25W(max.)

제품특성